User Manual

Universal Guide for Signal Jammers

⚠️ Critical Warning Before Initial Use

Never turn on the device without the antennas properly attached! If you activate the jammer without the antennas, the generated high-frequency power (totaling 12 W in this case) will not be radiated into the surrounding space; instead, it will reflect back into the power amplifiers, causing immediate and irreversible damage to the device.

Technical Specifications (Varies by model)

•	Frequency Bands: Independent bands covering 5G, 4G, 3G, 2G (GSM/CDMA), Wi-Fi (2.4G and 5.8G), and GPS (703–5900 MHz).
•	Output Power: Total power approx. 12 W (approximately 1 W per channel).
•	Jamming Range: 5 to 30 meters (depending on the strength of the local carrier signal).
•	Power Supply: Integrated lithium battery providing approximately 1 to 1.5 hours of operation.

Setup Procedure:

1.	Attaching Antennas: Each antenna and each connector on the device housing is marked with a number or a specific frequency band. Screw each antenna onto its corresponding connector (e.g., attach the antenna labeled "GPS" to the GPS connector).

2.	Tightening: Tighten the antennas firmly, but use care to avoid damaging the threads. 3.	Charging: Before using the device for an extended period for the first time, charge it fully using the supplied power adapter (or a 12V car charger). During charging, the LED indicator may glow red/orange; it will turn green once charging is complete.
4.	Turning On: Set the main power switch to the ON position. The integrated cooling fan should activate.

5.	Selective Jamming (DIP Switches): Most models in this series feature recessed DIP switches located on the side of the unit, near the individual antennas. These allow you to enable or disable specific frequency bands (e.g., only GPS or only Wi-Fi) as needed. They are set to the "off" position for transport; slide them to the left to turn them on. When the device is powered on, a green LED lights up next to these switches.

Maintenance and Safety
•	Cooling: The body of the jammer becomes significantly hot during operation. Do not cover the ventilation openings, and do not leave the device inside closed bags or cases while it is active.
•	Battery: To preserve battery life, do not leave the battery in a deeply discharged state for long periods.
